

**DS-PD2-T10AME-EH**

**Outdoor Dual-Tech Detector**

|  |  |
| --- | --- |
| The DS-PD2-T10AME-EH is a high security outdoor detector, combining established and patented technologies such as Tri-Digital Detection Signal Processing and Tri-Anti-Mask Technology which have been adapted to enhance performance in extreme outdoor conditions. |  |

**AVAILABLE MODEL**

|  |  |
| --- | --- |
| DS-PD2-T10AME-EH | Outdoor Dual-Tech Detector |
| DS-PDB-EX-Wall bracket | Wall bracket (Need to order separately )  |
| DS-PDB-EX-Adapter | Extend coverage to 90 degrees (Need to order separately, using together with DS-PDB-EX-Wall bracket) |
| DS-PDB-EX-Fixed bracket | Add two detectors back to back to create 20m perimeter protection (Need to order separately) |

\*All bracket need to order separately.

**MAIN FEATURES**

* Microwave + two PIR sensors
* Weather Proof sealed optics
* Heavy duty ultraviolet filter
* 10m volumetric coverage
* Tri-Anti-Masking Technology
* Digital Temperature Compensation

**SPECIFICATION**

|  |
| --- |
| **Outdoor Dual-Tech Detector** |
| **Detection Range** | 10m, detection angle: 90° |
| **Detection Speed** | 0.25m/s ~ 2.5m/s |
| **Animal Immunity** | 10kg |
| **Power Supply**  | 9-16V DC 13.8V DC typical |
| **Operation Temperature** | -25℃ ~ +60℃ |
| **Dimension(H\*W\*D)** | 188mm\*84mm\*77mm |
| **Weight** | 300g |
| **Installation Environment** | Outdoor |
| **Installation Height** | 1.8-2.4m |